Jesus Gutierrez

INSY 3303-002

Ch 7 Lab

1. A screen shot of a computer

   Description automatically generated
2. The 2 main channels used were 2.4 ghz and 5 ghz. The fastest signal on display was -29 dBm, while the slowest was -90 dBm. At -90 dBm, a connection is normally considered completely disconnected.
3. All the networks in my screenshot were password secured. Using WPA2.
4. I inspected local wireless networks in the residential neighborhood where I live. All the networks I inspected were password protected which is a good thing if powerful passwords are used. I am sure the case is very different in public areas that use public networks that aren’t password protected.